This package is intended for Anet A8 printer owners with Anet V1.0 Board and 5 buttons + 2004 LCD panel

---- How to upload repetier from source (and be able to customize it) ---- 

- Open arduino.exe located in "arduino-1.6.3" folder
- Open sketch and open repetier.ino located in folder Repetier-Firmware-5Keys-Anet-V1.0\Repetier
- In tools choose the "Anet V1.0" board (basically a sanguino, but renamed to avoid errors)
- Upload !

By default this firmware sets higher accelleration in lcd menu go into configuration and lower it to 100 or 200 instead of 400
Other features works flawlessly

---- How to restore original Anet V1.0 board firmware ---- 

- Go into Original-Anet-Board-Firmware folder and follow instructions found in "Firmware Upgrade.pdf"


Credits go to orignal Repetier authors and Hally who made the modifications to support the "5 keys"

