Arduino

Reference Language | Libraries | Comparison | Changes

## const keyword

The const keyword stands for constant. It is a variable qualifier that modifies the behavior of the variable, making a variable "read-only". This means that the variable can be used just as any other variable of its type, but its value cannot be changed. You will get a compiler error if you try to assign a value to a const variable.

Constants defined with the const keyword obey the rules of variable scoping that govern other variables. This, and the pitfalls of using#define, makes the const keyword a superior method for defining constants and is preferred over using #define.

#### Example

    const float pi = 3.14;
    float x;

    // ....

    x = pi * 2;    // it's fine to use const's in math

    pi = 7;        // illegal - you can't write to (modify) a constant

#### #define or const

You can use either const or #define for creating numeric or string constants. For arrays, you will need to use const. In general const is preferred over #define for defining constants.

See also:

- #define
- volatile

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- Careers